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Question 1 I cant remember the answer I chose
Question 2 16bit adder blab la bla answer is 64mb
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You have now completed TMA1 for CIT309: Computer Architecture
You scored a total of 10 out of 10!
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