


CIT311 TMA1 QUESTIONS & ANSWERS

1. Which layer of the OSI model does a bridge operate on? Network Layer (B)
2. In _ operation, both stations may transmit simultaneously. Full Duplex (C)

3. Which layer of the OSI model does an intelligent switch operate on? Layer 4 (C)

4. __ signal takes on continuous values on some interval. Analog (C)

5. Sub-netting was developed to solve the following problems except? Cost of network devices (D)

6. FTP applications are considered at which level of the OSI model? Layer 7 (A)

7. What is the main function of the routing algorithm? It decides which output line an incoming packet should be transmitted to (B)

8. EGP is handled by which network operating system? TCP/IP (C)

9. __ occurs between transmitters and receivers over some transmission medium? Data Transmission (A)

10. Language rules and regulations are considered at what level of the OSI model? Layer 6 (D)
