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                       Chapter – 3
2.  HYDROSTATICS
 2.1 Introduction
Hydrostatics deals with the study of fluids at rest or moving with uniform velocity as a solid body, so that there is no relative motion between fluid elements (or layers). There is no shear stress in a fluid at rest. Hence, only normal pressure forces are present in hydrostatics.

Engineering applications of hydrostatics principles include the study of forces acting on submerged bodies such as dam faces, gates & others and the analysis of stability of floating bodies. 

2.2 Hydrostatics Pressure at a point :- 

The pressure at a point is the limit of ratio of the normal force on infinitesimal area dA.

  i. e  P  =   
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No tangential stresses can exist in a fluid at rest. At a point a fluid at rest has the same pressure in all directions. This is known as PASKAL’S LAW. This means that an element having very small area (
[image: image2.wmf]d

A) in the fluid, free to rotate about its center when submerged in a fluid at rest, will have a force of constant magnitude acting on either side of it, regardless of its orientation.

Consider a small wedged- shaped fluid element at rest. The thickness of the element perpendicular to the plane of the drawing is assume to be unity (
[image: image3.wmf]d

z=1) 
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Fig.2.1 Small wedged- shaped fluid element       
The weight of the fluid element is, 

                               = (area of triangular element *depth)*specific weight 
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                 Fx =Px* (y*1
                 Fy = Py* (x*1
   ( X = (Y = very small number 

Since there is no shear force, the only forces acting on the wedge are the normal surfaces forces & gravitational force.

The fluid prism (element) is in equilibrium,   i.e. 
   

[image: image7.wmf](

)

0

0

.

1

.

2

.

2

1

*

.

.

.

cos

1

.

1

*

.

0

)

0

(

2

.

2

...

..........

0

2

1

*

.

.

.

1

*

.

0

=

=

=

-

-

Þ

=

=

=

÷

÷

ø

ö

ç

ç

è

æ

=

-

Þ

=

å

å

y

y

y

x

y

x

l

x

y

y

x

x

y

x

l

l

y

X

x

a

a

P

P

F

a

a

Sin

P

P

F

r

d

d

d

d

g

q

d

d

r

d

d

q

d

d

l


Using geometric relations: 

.
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We obtain: 

Px. ( y  - P
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As 
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is infinitesimal of higher order, it may be neglected. 
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It can also be proved that PZ = P
[image: image15.wmf]l

, by considering a three dimensional case. The results are independent of ( hence the pressure at any point in a fluid at rest is the same in all directions. 

2.3 Basic Equation of Hydrostatics
The basic equation of Hydrostatics may be derived by considering the infinitesimal fluid parallepiped in a static fluid shown in fig. 2.2. below.
[image: image16.jpg](p+32s2)8x5y





Fig 2.2 A rectangular fluid parallelepiped
Assuming the density of the fluid ρ in the infinitesimal cube to be constant, the mass of the fluid is ρ.dx.dy.dz. Let the pressure variation in the x, y and z directions be 
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 respectively and let the entire fluid mass be subjected to acceleration of ax, ay, and az, in the x, y and z directions respectively.
Considering the equilibrium in the vertical (Z) direction:
[image: image18.jpg]+p dx.dy ~(P+S2 dz) dx.dy - pg dx dy dz

a,. pdxdydz = 0




which reduces to
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Similarly it can be shown that
                               [image: image20.jpg]



The total change in pressure is given by the total differential as follows:
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 …………………. 2.4

Equation 2.4 is the basic equation of fluid statics applicable for both compressible and incompressible fluids.
2.4 Variation of Pressure with Elevation in a Static Incompressible Fluid
For a fluid at rest and subjected only to gravitational force, the accelerations ax, ay and az are zero. Eqn2. 4 thus reduce to:
                             [image: image22.jpg]dp = -pg dz



          ……………………. 2.5
Equation 2.5 holds true for both compressible and incompressibile fluids. However for homogeneous and incompressible fluids, ρ is constant and eqn 2.5 may be integrated to give;
[image: image23.jpg]pP=-pgz+cC



                           2. 6

where c is a constant of integration and is equal to the pressure at z = 0. In hydrostatics the law of variation of pressure with depth is usually written as;
[image: image24.jpg]p = pgh+p,



                           2.7

In Equation 2.7, h is measured vertically downward ( i . e. h =-z) from a free surface, p is the pressure at a depth h below the free surface and po, is the pressure at the free surface.
Equation 2.7 shows that for a fluid at rest, the pressures at the same depth from the free surface are equal. Hence in a homogeneous continuous fluid a surface of equal pressures is a horizontal plane.
[image: image25.jpg]



Fig 2.3

Consider two points (1) and (2) at a depth of h1 and h2 in a tank containing a liquid, with density ρ, at rest as shown in Figure 2.3. The pressure at (1) is p1 = p0 + pgh1. The pressure at (2) is p2 = p0 + pgh2. If h1 = h2, then p1 = p2.

For h1 > h2, the pressure difference between (1) and (2) is p1 - p2 = ΔP = ρghl - ρgh2 = ρg(h1 - h2) = ρgΔz.
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 is the pressure difference between (1) and (2) expressed as a height of the liquid. This difference is also refered to as the pressure head difference. Thus, by dividing a pressure by the specific weight γ = ρg of a fluid, the pressure can be expressed as height of fluid column.
2.5 Variation of Pressure with Elevation in Static Compressible Fluids
Since density varies with pressure in compressible fluids, the relation between density and pressure must be known in order to integrate the basic equation of fluid statics and obtain expressions for the variation of pressure with elevation in compressible fluids. The relation between pressure and density is dependent on the prevailing conditions. These conditions are; Constant temperature (i.e. isothermal), adiabatic and constant temperature gradient conditions.
Isothermal Condition: The relation between pressure, density and temperature for constant temperature condition is given by the perfect gas law: PV = mRT, 
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Substituting this in the basic equation of hydrostatics i.e. Equation 2.5 

[image: image29.jpg]


:
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Integrating from p = p1 where z =z1 to p = p2 where z = z2
[image: image31.jpg]



Or           [image: image32.jpg]P./p, = exp (-g/RT) (2, - z,)



                                           2.8

Adiabatic Condition: Under adiabatic condition the relationship between pressure and density is given by p/ρk = constant = p1/ρ1k,
So that,
                          [image: image33.jpg]P =p; (p/p)Y*




Substitution of the above in the basic equation 2.7 gives:
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[image: image35.jpg]or dz = -(p}’*/p,g) .p"*.dp




Integrating from p = p1 when z = z1 to p = p2 when z = z2,
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The above may be written as:
[image: image38.jpg]= ~(k/ (k-1)) (p;/ @) {(p;/p,) ¥ 1/ - 1}





[image: image39.jpg]or, since p,/p, = RT for any gas,




[image: image40.jpg]2y - 2y = (k) gy RTyyq {(Pal ) 7% - 1)
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                                   2.9 

In the above equation, T is absolute temperature in ok, R = 288J kg-1 k-1 = 288 m2/s2 0c, and k = 1.4 for adiabatic condition.
The temperature lapse rate 
           - the rate of change of temperature with altitude 
           - can be found for adiabatic conditions as follows:

Substituting the characteristic equation, ρ = p/RT in Equation 2.2 and rearranging,
[image: image42.jpg]dz = - (RT/gp) dp




[image: image43.jpg]For adiabatic condition, p/p* =p,/py , and since p/p = RT ,




Substitution and rearranging gives:
[image: image44.jpg]p = p, (T,/T) K2R




Differentiating the above,
[image: image45.jpg]dp = -lk/ (1-k))p,. T¥/ SR g1/ aRgr




Substituting the values of p and dp in the equation for dz,
[image: image46.jpg]dz = k/(1-K)HR/g) dT




Therefore, the temperature gradient is given by:
[image: image47.jpg]dr/dz = -{(k-1) /Kl (g/R)




Constant Temperature Gradient Condition: Assuming that there is a constant temperature lapse rate (i.e. dT/dZ = constant) with elevation in a gas, so that its temperature drops by an amount δT for a unit change in elevation, then if T1 = temperature at elevation Z1, then T = temperature at elevation Z is given by:
[image: image48.jpg]T, - 3T (2 - 2,)




Putting this in Equation 2.7 and noting that p/ρ = R T,
[image: image49.jpg]dp/dZ = -pg/RT




         [image: image50.jpg]dp/p

(-g/RT)dz




Substituting the above value of T,

[image: image51.jpg]dp/p = -lg/ (R(T, - 8T(Z~

,))) 1dz




[image: image52.jpg]Integrating the above between limits P,and P, and 2, and Z,,




[image: image53.jpg]p,/p, =1 - (3T/T)) (2,-2,) 19"




On the average, there is a temperature gradient of about 6.50C per 1000 m in the atmosphere i. e. δT = 6.5 0c per 1000 m = 0.00650c.m-l.
2.6 Absolute & Gage Pressure

Pressure values may be expressed with reference to any arbitrary datum (level) it is usually expressed w. r .t absolute zero (perfect vacuum & local atmospheric pressure). When the reference is absolute zero, the pressure is called Absolute pressure; if the pressure is measured w. r .t local atmospheric pressure it is called Gage pressure.
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Fig 2.4 Pressure and Pressure datum
Absolute pressure is always positive, but gage pressure is positive if the prevailing is greater than patm & negative if prevailing pressure is less than patm 

     Pabs =   Patm + P gag …………….   2.9 

Atmospheric pressure is also called Barometric pressure simple Barometer (mercury barometer) consists of an inverted tube closed at one end& immersed in a liquid with the open and down 

If the air is completely exhausted from the tube, the atmospheric pressure on the surface of the liquid in the container forces the liquid to rise in the tube to a height y & the only pressure on the liquid surfaces in the tube is vapor pressure of the liquid, Pv

P0  =  PA =  Patm (from Pascal’s law)

From the condition of static equilibrium of the liquid above O is the tube of cross- sectional area A 

P atm A – Pvapors* A - ( A y = 0  


[image: image55.wmf]Þ

  P atm =    ( y   + Pvap

But vapor is very small compared to Patm & it can be neglected ,Pv – for mercury is 0.173 Pa at 20c0 but for water it shouldn’t be neglected because Pv – for water is 2.447 K Pa at 2002 

Thus P atm =   ( y ……………………………………………….. 2. 10a
Y =   P atm / ( ………….. 2.10b
(Pressure head) 

If the liquids with low specific weight are used, Y – shall be excess very high. For example for water barometer, Y = 10 .33 m at sea level and for mercury barometer, y = 0.76 m = 760 mm at s. e 

2.5  Measurement of pressure:-

In practice, pressure is always measured by the determination of a pressure difference More usually the difference determined is that between the pressure of the filed concerned & the prevailing   atmospheric pressure. This is the difference normally recorded by the pressure page & is known as gage pressure. 

There are so May ways which pressure in a fluid may be measured 

I. Bourdon gage 

The is a typical devices used for measuring gage pressures. Where high precision is no required a pressure difference may be indicated by the deformation of an elastic solid. It consists of a curved tube of elliptical cross- section at one end. The closed end is free to move while the open end through which the fluid enters is rigdely fixed to frame. 

The reading zero (0) implies the is no difference in pressure in the atmosphere & liquid 

· pressure greater than atmospheric straighten the tube for pressure less than atmospheric, the tube tends to coil again 

[image: image56.jpg]



Fig. 2.5   Bourdon gage
II. Piezometer
· It is used to measure moderate positive pressure of liquids it consists of a simple transparent tube open to atmosphere, in which the liquid can freely rises without over flowing. The height of the liquid will rises in the tube indicates the pressure head. To reduce capillary effect the diameter of the tube should be greater than 12 mm 

· it the pressure of a flowing fluid is to be measured, the hole must be drilled absolutely normal to the interior surface of the wail, and the piezometer tube or the connection for any other pressure measuring device must not project beyond the surface Also, the hole  should be small, preferably not larger than 3 mm diameter it r   is the sp. Wt  of the liquid , then pressure at A gage pressure is  

                   PA    =    +  γ h (gage reading) 
[image: image57.jpg]



 III. MANOMETERS: -
            Simple Manometer
Manometers are devices in which columns of a suitable liquid are used to measure the difference of pressure between certain point& the atmosphere, or between two points neither of which is necessarily at atmospheric pressure. They are suitable of measuring high pressure differences, both positive and negative in liquids & gases. 

Essentiality, a monometer is a piezometer with U bend tube in it in the bent, a denser fluid (usually mercury) is added. 

[image: image58.jpg]



Fig 2.6 The Simple manometer
Since in a continuous homogeneous fluid the pressure is the same at any two points of equal level, the pressure at K & L are equal 

When equilibrium condition is achieved: PK = PL 

           Pk    =  Patm + γM y1 = PL = PA + γN y2
            PA =  Patm + γM y1 -  γN y2                   
Differential Manometers:- 

A differential manometer (U – the manometer) determines the difference in pressures at two points A & B when the actual pressure at any point in the system can’t be determined 

[image: image59.jpg]



 Fig 2.7 Differential  manometer
At aquarium on K-L (horizontal plane)

PK = PL  

PA + γN y3 + γN y1 = PB  + γO (y1-y2) + γ m y2 

PA – PB = γO (y1-y2) + γ m y2 – (γN y3 + γN y1)
Example 2.1 

A closed tank is partly filled with water and connected to the manometer containing mercury (S = 13.6) as shown in the figure below. A gauge is connected to the tank at a depth of 4 m below the water surface. If the manometer reading is 20 cm, determine the gauge reading in N/ m2. What will be the gauge reading when expressed as head of water in m?
[image: image60.jpg]Mercury, ¥y




Solution 
[image: image61.jpg]Using the letter designation in the Figure, p, =Dpa

Py = P} - 0.20 vy
Po = Pgand Py = Pgug, = P+ 4 ¥,
P, = Py - 0.20y, + 4y,

=0 -0.20XY,.5, + 4y, = ¥,(-0.25, + 4)

9810 & (0.2 x 13.6 + 4)m = 9810(-2.72 + 4) N/m?
m

1

P, =9810 x 1.28 = 12556.8 n/M?*




Therefore, the gauge reading is 12556.8 N/m2

When expressed as head of water, the gauge reading will be
[image: image62.jpg]_ 12556.8 N/m?

9810 N/m?

=1.28m




Example 2.2 

A manometer is mounted in a city water supply main pipe to monitor the water pressure in the pipe as shown below. Determine the water pressure in the pipe.

[image: image63.jpg]



Solution
[image: image64.jpg]Ygg- 1 =P, +0.70 7,

Py =Ygy x 1= 0.7Y,+13.67, - 0.77,

"

12.9 y, = (12.9 x 9810) N/m?

= 1,2655 x 10° N/m = 1.24%atmospheres
(Note: 1 standard atmosphere = 1.01325 x 10°% N/m?)




Example 2.3

Calculate the pressure difference between points A and B in the differential manometer shown in Figure below. 

[image: image65.jpg]



Solution
[image: image66.jpg]Starting from A,

Py + (x - 0.5)y, + 0.6y, - 0.6 X 13.67, - X7, = P,
PA + xv, - 0.5y, + 0.67, - 8.16%, - XYy, = P,

P, - PB = (8.16 - 0.1)7, = 8.06y,

8.06 X 9.81 = 79.07 kN/m*




Example 2.4 

In the two compartments closed tank shown in Fig below, the pressure in the air in the left compartment is 26.7 kN/m2 while that in the air in the right compartment is 19.62 kN/m2. Determine the difference h in the levels of the legs of the mercury manometer. Specific gravity of mercury is 13.6.
[image: image67.jpg]



Solution 
Since the pressure in a static fluid is the same in a horizontal plane, PA = PB
[image: image68.jpg]P, =P +3.5xXy,=19.62 + 3.5 x 9.81 = 53.955kN/m’
Py =Pp+4.1%0.9y, +hx13.67,

-26.7 + 4.1 X 0.9 X9.81 +h x13.6 x 9.81
-26.7 + 36.20 + 133.42 h
=9.5 + 133.42 h
9.5 + 133.42 h = 53.955
Thus h = (53.955-9.5)/133.42 = 0.333 m
= 33.3 cm




2.6 Hydrostatic Forces on Surfaces
Plane and curved surfaces, immersed fully or partly in liquids, are subjected to hydrostatic pressure forces. It is, therefore, essential to determine the magnitudes, directions and locations of the hydrostatic pressure forces on surfaces as a first step in the analysis of the stability of a body fully or partly immersed in a liquid and in the design of hydraulic structures such as dams and gates.
2.6.1 Hydrostatic Force on Plane Surfaces
a. Horizontal Plane surfaces

The pressure intensity in a static fluid is the same at any two points in a horizontal plane surface. Therefore, a plane surface in a horizontal position at a depth h below the free surface in a fluid at rest will be subjected to a constant pressure intensity equal to (.h, where ( is the specific weight of the fluid. The total pressure force on a small differential area is given by:
[image: image69.jpg]



The total pressure force on the entire horizontal plane surface with area A will be
[image: image70.jpg]Ik
vhda
= vha





The force Fp acts normal to the surface and towards the surface. Since the pressure intensity is distributed uniformly over the plane surface, the total resultant force Fp acts through the centroid of the area and h = [image: image71.jpg]


 where [image: image72.jpg]


 is the depth from the free surface to the centroid. Thus, for horizontal plane surfaces, the centre of pressure C coincides with the centroid G. The centre of pressure is the point on the immersed surface at which the resultant pressure force on the entire area is assumed to act.
b. Vertical Plane Surface
Consider a plane vertical surface of area A immersed vertically in a liquid (Fig. 2.8). Since the depth from the free surface to the various points on the surface varies, the pressure intensity on the surface is not constant and varies directly with depth. Figure 2.8
[image: image73.jpg]o ===
0
he
——6
-4——1tc
;
t





Fig 2.8 

Consider also a narrow strip of horizontal area dA, shown shaded in Fig. 2.8, at a depth h below the free surface. The pressure intensity on this area dA is (.h and is uniform. The total pressure force on one side of the strip is thus

[image: image74.jpg]



Or                     [image: image75.jpg]



where [image: image76.jpg]


 is the depth from the free surface to the centroid G of the area. Thus, as for a horizontal plane area, the magnitude of the resultant hydrostatic pressure force on a vertical plane area is obtained by multiplying the pressure intensity at the centroid G, i. e ([image: image77.jpg]


by the total area A.
If the vertical area is not of a regular shape, the area may be divided into a finite number of small regular areas and the total hydrostatic pressure force determined as the sum of the pressure forces acting on these small areas.
The total pressure force Fp acts normal to the vertical plane area and towards the area through the centre of pressure C. Since the pressure distribution on the area is not uniform, the centre of pressure and the centroid will not coincide. The depth hc to the centre of pressure may be obtained from the principle of moments. The moment of the elementary force dFP, acting on the area dA (Fig. 2.8) about axis 0-0 on the free surface is
[image: image78.jpg]dM = dF,.h = (y.h dA)h




The total moment of all elementary forces on the whole area is:
[image: image79.jpg]M=fdM=fy.h‘.dA




From the principle of moments, the sum of the moments of a number of forces about an axis is equal to the moment of their resultant about the same axis. Thus:
[image: image80.jpg]



The term [image: image81.jpg][h?da



may be recognized as the second moment of area about the free surface i.e. [image: image82.jpg]


.
[image: image83.jpg]



i.e, using the parallel axis theorem of second moment of area,
[image: image84.jpg]I+ A(h)?





Where IG is the second moment of area about the axis parallel to 0-0 and passing through the centroid G. Therefore,
[image: image85.jpg]_ ¥+ AR)?)
y.h.A





Or                                             
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Thus, the centre of pressure C for vertical plane area is below the centroid by an amount equal to:                              

                                                 [image: image87.jpg]1./Ah




The moment of Fp about the centroid is:
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, which is independent of depth of submergence.
c. Inclined Plane Surface 
The analysis of the hydrostatic force on an inclined plane surface will be made by considering a plane surface of arbitrary shape and total area A inclined at an arbitrary angle θ to the free surface as shown in Fig. 2.9. AB is the trace of the inclined surface the extension of which intersects with the free surface a 0. hc and hp are the depths from the free surface to the centroid C and centre of pressure CP of the area respectively. yc and yp are the corresponding distances from 0 to C and CP respectively, measured along the inclined surface. It is required to determine the magnitude, direction and line of action of the resultant hydrostatic force Fp acting on one side of the area.
[image: image89.jpg]Free Surface





Fig 2.9 Hydrostatic force on an inclined plane surface

The magnitude of the force dFp acting on an elementary area dA at a depth h below the free surface is given by

[image: image90.jpg]p.dA = pgh.dA = pg.ysin® dA



                              
The force dFp acts normal to the plane surface. The resultant hydrostatic force Fp is the sum of all elementary forces dFP which are parallel to each other.
[image: image91.jpg]Thus F, = [dF, = pg Sin® [yda




But [image: image92.jpg]


is the first moment of area A about axis through 0 and is equal to yc.A and since yc Sin θ =hc the above equation for Fp becomes: 

[image: image93.jpg]=y Sindy _A=vh_ A





(hc is the pressure intensity at the centroid of the inclined plane area. This shows that the magnitude of the resultant hydrostatic force on an inclined plane area is equal to the product of the area and the pressure intensity at the centroid of the area. The force Fp acts normal to the plane surface and towards the surface.
The resultant force Fp acts through the centre of pressure CP of the submerged plane area. The location of CP is determined using the principle of moments for a parallel force system. In Fig. 2.9 let the axis through 0 coinciding with the free surface be the axis of moments. 
The moment of force dFp about this axis is equal to dMo which is given by
[image: image94.jpg]dM, = y.dF_ = y.pg.y Sin dA = pg Sinf y“dA




The moment of the resultant force Fp about the axis of moments will be equal to the sum of all elemental moment dMo. i.e.
[image: image95.jpg]F, V., = [aM, = pg 5iné [ y®dA = v Sin® I,




Where [image: image96.jpg]


is the second moment of the plane area about axis 0-0.

[image: image97.jpg]Sin® I, 5inb I, 2
Thus  yg, = 1520 Teo . ¥ 5200 Top | foo
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Using the parallel axis theorem,

[image: image98.jpg]



Where Ic is the second moment of area about an axis parallel to 0-0 and passing through the centroid c.
Thus            [image: image99.jpg]Vep =

I +yiA

VA




This shows that the centre of pressure is always below the centroid of the area. The same has been shown for vertical plane surfaces.
The depth of the centre of pressure below the free surface is hcp = ycp sinθ. Substituting this and the value of yc = hc/Sinθ, the following equation is obtained for the depth to the centre of pressure.
[image: image100.jpg]I, Sin% 6




When the surface area is symmetrical about its vertical centroidal axis, the centre of pressure CP always lies on this symmetrical axis but below the centroid of the area. If the area is not symmetrical, an additional coordinate, xcp, must be fixed to locate the centre of pressure completely.
Referring to Figure 2.10, and using moments,
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Fig 2.10 Centre of pressure of an asymmetrical plane surface
d. Hydrostatic Force on Curved Surfaces
The total hydrostatic force on a curved surface immersed in a liquid cannot be directly determined by the methods developed for plane surfaces. For plane surfaces, the pressure forces on elementary areas act perpendicular to the surface and hence are parallel to each other. Consequently, it is easier to obtain the resultant force by a simple summation of the elementary forces. In the case of a curved surface each elementary force acts perpendicular to the tangent of the elementary area and because of the curvature of the surface the direction of each elementary force is different.

As a result, the usual procedure is to determine the horizontal and vertical components of the resultant force and then add them vectorially to obtain the magnitude, direction and location of the line of action of the resultant hydrostatic force.
Consider the curved surface BC of unit width shown in Figure 2.10.
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Fig 2.10 Hydrostatic force components on curved surfaces.
The elementary force dF acting on the elementary area dA has a horizontal component dFx and a vertical component dFy. The pressure intensity on dA is ρgh.
                              The total hydrostatic force on dA = dF = ρgh dA
                              The horizontal component of dF = dFx = ρgh dA Cosθ
                              The vertical component of dF = dFy = ρghdA Sinθ
But dA Cosθ = dAv = the projection of dA on the vertical plane and dA sinθ = dAh = The projection of dA on the horizontal plane.
The components of the total hydrostatic force in the x and y directions are Fx and Fy respectively and are given by:
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Where: Av is the projection of the whole curved surface BC on the vertical plane, i.e. BD           

           dV is the volume of the water prism (real or virtual) extending over the area dA to         

                 the free surface.
[image: image108.jpg]



Thus :

The horizontal component, Fx, of the resultant hydrostatic force on a curved surface BC is equal to the product of the vertically projected area of BD and the pressure intensity at the centroid of the vertical area BD. The Force Fx passes through the centre of pressure of the vertically projected area BD.

The vertical component, Fy, of the resultant hydrostatic force on a curved surface BC is equal to the weight of the water (real or virtual) enclosed between the curved surface BC, the vertical BD and the free surface CD. The force component Fy acts through the centre of gravity of the volume.
The resultant force F is given by:
[image: image109.jpg]



F acts normal to the tangent at the contact point on the surface at an angle a to the horizontal, where
[image: image110.jpg]« = tan"1l (f,/F,)




Exercise 

1. A vertical rectangular gate AB shown in Figure below has a width of 1.5 m. The gate is hinged on its upper edge at A.
            Determine the moment M at A required to just hold the gate from opening.
[image: image111.jpg]



2. The 2 m wide and inclined rectangular gate AB shown in Figure below is hinged at B. The gate is unifrom and weighs 24 kN.
            Determine

            a) The magnitude and location of the hydrostatic forces on each side of the gate.

            b) The resultant of the hydrostatic forces.

            c) The force F required to just open the gate.
[image: image112.jpg]



3. A triangular opening in the form of an isosceles triangle, with dimensions shown in Figure below and with its axis of symmetry horizontal, is closed by a plate. Water stands at 9 m from the axis of symmetry. Determine the resultant hydrostatic force on the plate and its centre of pressure.
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4. A vertical, symmetrical trapezoidal gate with its upper edge located 5 m below the free surface is shown in Figure below,

            Determine the total hydrostatic force and its centre of pressure.
[image: image114.jpg]



5. An inverted semicircular plane gate shown in Figure below is installed at 450 inclination as shown. The top edge of the gate is at 3 m below the water surface. Determine the total hydrostatic force and the centre of pressure.
  [image: image115.jpg]



5. A log hods water as shown in Figure below. Determine

   a) The force pushing against the obstruction (dam) per metre length of log.

   b) The weight of the log per metre length

   c) The specific gravity of the log.
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