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           Alternating current (a.c) circuit
   A.c generator is the source of alternating current  
  Alternating current (a.c) :- oscillation of current i.e the current that moves back and forth.
  Alternating current is generated by the induced electromotive force,Ԑ in the generator. The induced 
electromotive(voltage) and current are expressed in sinusoidal function. Based on Lenz’s law, the  induced voltage and current in the generator are in phase and expressed in the same manner as
       V=V0sin       and   I=I0sin    where V and I are instant voltage and current respectively.
                                                                                         V0, I0 --- maximum (pick) values of voltage and current.
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)    Expressions of the generated voltage and current by the a.c generator are the same in a resistor 
    connected to the a.c circuit.
     Like any other forms of energies, electric energy
      is also expressed in terms of average work done
     to induce voltage as well as current. Then the voltage and current expressed as average values.
    The values are named as root mean square (rms) values. The rms value is the square root of square 
      of average value i.e     .  They are derived from average electric 
    power,          
                                                            
                                                 
               Where Vrms ---rms of voltage 
                                                                                                  Irms  ---rms of current

       A.C circuit :-path of electric current connected to a.c source. 
           The a.c circuit contains different electric elements separately or commonly according to the
           applications. In the circuit, there can be energy dissipative devices or storage devices.
          The a.c circuit is named as oscillatory circuit. Property of voltage and  current in each electrical 
          device by sinusoidal function and phase  diagras.
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)    Resistive circuit (R—circuit) and alternating current (a.c)
     Voltage and current are in phase.
       V=V0sinꙍt     and     I=I0sinꙍt  
      Value of the resistance the same at any instant of V and I.
            
            The sine function and phase diagrams of V and I are as follow.
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  The resistor resists current by producing resisting voltage. Then the dissipative power known as
           real power in the a.c circuit is expressed as :
                P=VrmsIrms ------
      eg. Pick values of voltage and current of a.c source in a resistive circuit are 220V and 30A . Find 
             dissipative power and the resistance.
   Solution   
                            
                                                
       Capacitive circuit (C—circuit) and alternating current   
           Capacitor is energy storage device. It is charged and discharged. Then the current flows in the
 (
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C
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)            capacitive circuit with change of polarities on the two
            parallel plates of the capacitor. Energy (voltage)  is stored 
           on  the capacitor, after current reaches the capacitor. Then    
.          current comes to the capacitor before the voltage. The process
           shows current and voltage are out of phase by . The phase is called 
            phase lead since current leads voltage. Sinusoidal functions of voltage (V) and current (I)
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Sinusoidal graphs of current and voltage
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)          are expressed as follow.  
                     I=I0sinꙍt
                 V=V0sin(ꙍt+)
                *  V=V0sinꙍt
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)	Phaser diagram of
	current and voltage  
	are shown as follows.

  The capacitor opposes change of current in the a.c circuit to keep stored charge as it is or fluctuation
  of stored energy in the capacitor. This opposition against change of current by the capacitor is known
  as capacitive reactance (Xc). It is not fixed like resistance. Its value is determined on the bases of
   complex number (Z=a+bi). Since it has no real, it is expressed in terms of imaginary value i.e ( Z=Xci)
  The capacitive reactance (Xc) is derived as follows starting with definition  of current.
       
     
          -------------   I0=CꙍV0    -------------       
     In terms of Ohm’s law, is the resistance,R . Now    is equivalent to the resistance and named as
     capacitive reactance,Xc. Therefore, Xc= . This is definition of capacitive reactance.
 eg. 400µF capacitor is connected an a.c source with 50Hz frequency. What will be the capacitive 
        reactance?  ()
 Solution:-    Xc=     ,          where ꙍ=2
                            
                            
          NB – Unit of reactance is also ohm () similar to a resistance.
  Inductive circuit (L-circuit) and alternating current (a.c)
 (
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)    In the inductor voltage is produced first to store energy. Then
     voltage leads current by a phase difference of   . The phase
      difference in the inductor is said to be phase lag since the
     current lags in the inductive circuit.
      voltage and current in the inductive circuit are expressed  as
       
       The sinusoidal functions of voltage and current and their phase diagrams are shown as follow.
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         In the a.c circuit the inductor is magnetized and demagnetized. This is done due to opposing of
        change of current  by the inductor. Opposing of current the inductor is called inductive reactance,XL.
        Like capacitive reactance it is expressed a complex number (Z=a+bi). The real part is zero. Then it is 
       stated as             Z= X Li .
       The value of XL is derived using     .
                                            
                                           
                                           
      Lꙍ is equivalent to the resistance,R  since . Then Lꙍ defines the inductive reactance,XL.
       Therefore, XL=Lꙍ   or  XL=2L  since ꙍ=2 . The is expression of the inductive reactance.
     eg. A 0.6H of an inductor is connected to an a.c source with 50Hz frequency. What is the inductive 
          reactance?
      Solution:-     XL=Lꙍ=2L
                                 XL=2
                                Hz
