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Mini project

# Analyze the building skeletal (beams and frames by using kani method and moment distribution method in both sway and non- sway conditions.
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	Material 
	Group

	Concrete slab (200mm)
	1
	2

	Beam (30cm *30cm)
	Lateral load on axis AE 10KN, 8KN, and 5KN above the ground level
	Lateral load on axis KP 10KN, 7KN, and 5KN above the ground level

	Unit weight of concrete = 25KN/m3
	Unit weight of soil = 19KN/m3
Angle of internal friction = 300
Below ground level
	Unit weight of soil = 18KN/m3
Angle of internal friction = 280
Below ground level
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