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Mode: Simplex Mode

Reason 1: In this case unidirectional communication is required as broadcast sends
signals to display screen and there is no Need to send back signals from screen.

Reason 2: Using simplex mode whole bandwidth can be used during transmission,
and | think for live transmission simplex mode is best choice.
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